{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F"]
[]
[]
[]
[]
["","","","","FVXS25FV1B","FVXS35FV1B","FVXS50FV1B"]
["Sound pressure level","Heating","High","dBA","38","39","45"]
["","","Silent operation","dBA","23","24","32"]
["","","Low","dBA","26","27","36"]
["","Cooling","Silent operation","dBA","23","24","32"]
["","","Low","dBA","26","27","36"]
["","","High","dBA","38","39","44"]
["","","Nom.","dBA","32","33","40"]
["","Cooling","Nom.","dBA","32","33","40"]
["Standard Accessories","دليل التركيب","","","1","1","1"]
["","دليل التشغيل","","","1","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","1","1","1"]
["","البطاريات","","","2","2","2"]
["","حامل جهاز التحكم عن بعد","","","1","1","1"]
["","خرطوم الصرف","","","1","1","1"]
["","مرشح ضخ الهواء","","","","1","1"]
["","شريط عازل حرارياً","","","2","2","2"]
["أنظمة التحكم","Infrared remote control","","","ARC452A1","ARC452A1","ARC452A1"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.5","9.52","12.7"]
["","Drain","","","20","20","20"]
["Sound power level","التبريد","","dBA","52","52","60"]
["","التدفئة","","dBA","52","52","60"]
["Dimensions","Unit","العرض","mm","700","700","700"]
["","","العمق","mm","210","210","210"]
["","","الارتفاع","mm","600","600","600"]
["الغلاف","اللون","","","White","White","White"]
["الوزن","الوحدة","","kg","14","14","14"]
["Power supply","الطور","","","1~","1~","1~"]
["","Frequency","","Hz","50","50","50"]
["","الاسم","","","V1","V1","V1"]
["","Voltage","","V","220-240","220-240","220-240"]
["Standard Accessories","مرشح تنقية الهواء","","","2"]
["Notes","","","","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","(4) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]