{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MKS-E"]
[]
[]
[]
[]
["","","","","","3MKS50E2V1B","4MKS58E2V1B","5MKS90E7V3B"]
["الأبعاد","الوحدة","","الارتفاع","mm","735","735","770"]
["","","","العرض","mm","936","936","900"]
["","","","العمق","mm","300","300","320"]
["الوزن","الوحدة","","","kg","49","49","69"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46"]
["Sound pressure level","Cooling","","Nom.","dBA","46","46","48"]
["سائل تبريد","النوع","","","","R-410A","R-410A","R-410A"]
["","السعة","","","kg","2.0","2.0","2.95"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","50","50","75"]
["Piping connections","Additional refrigerant charge","","","kg/m","Chargeless","Chargeless","0.02 (for piping length exceeding 65m)"]
["","Level difference","IU - OU","Max.","م","15","15","15"]
["","","IU - IU","Max.","م","15","15","7.5"]
["Standard Accessories","دليل التركيب","","","","1","1","1"]
["","سدادة المصرف","","","","1","1"]
["","لوحة ضبط اتجاه الهواء","","","","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230","230"]
["Notes","","","","","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب المكافئ: 7.5 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب المكافئ: 7.5 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب المكافئ: 7.5 م"]
["Standard Accessories","مجموعة المخفض","","","","","1","1"]