{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MKS-F"]
[]
[]
[]
[]
["","","","","","4MKS75F2V1B"]
["Sound pressure level","Cooling","","Nom.","dBA","48"]
["Standard Accessories","Installation manual","","","","1"]
["","سدادة المصرف","","","","1"]
["","مجموعة المخفض","","","","1"]
["","لوحة ضبط اتجاه الهواء","","","","لوحة ضبط اتجاه الهواء"]
["Refrigerant","Charge","","","kg","2.3"]
["","النوع","","","","R-410A"]
["Piping connections","Level difference","IU - IU","Max.","م","15"]
["","","IU - OU","Max.","م","15"]
["","Additional refrigerant charge","","","kg/m","Chargeless"]
["Sound power level","التبريد","","","dBA","61"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","936"]
["","","","العمق","mm","300"]
["","","","الارتفاع","mm","735"]
["الوزن","الوحدة","","","kg","57"]
["Power supply","الطور","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230"]
["Notes","","","","","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب: 5 م"]