{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MKS-G"]
[]
[]
[]
[]
["","","","","","2MKS40G2V1B","2MKS50G2V1B"]
["Sound pressure level","Cooling","","High","dBA","47","48"]
["Standard Accessories","Installation manual","","","","1","1"]
["","حقيبة المسامير اللولبية","","","","1","1"]
["","مجموعة المخفض","","","","","1"]
["","لوحة ضبط اتجاه الهواء","","","","لوحة ضبط اتجاه الهواء","لوحة ضبط اتجاه الهواء"]
["Refrigerant","Charge","","","kg","1.20","1.60"]
["","النوع","","","","R-410A","R-410A"]
["Piping connections","Level difference","IU - IU","Max.","م","7.5","7.5"]
["","","IU - OU","Max.","م","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)"]
["","طول الأنابيب الإجمالي","النظام","فعلي","م","30","30"]
["Sound power level","التبريد","","","dBA","62","63"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","765","765"]
["","","","العمق","mm","285","285"]
["","","","الارتفاع","mm","550","550"]
["الوزن","الوحدة","","","kg","38","42"]
["Power supply","الطور","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب: 5 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب: 5 م"]