{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RKS-F"]
[]
[]
[]
[]
["","","","","","RKS60F3V1B","RKS71FAV1B"]
["Sound pressure level","Cooling","","High","dBA","49","52"]
["","Night quiet mode","","Level 1","dBA","46","49"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual"]
["Refrigerant","Charge","","","kg","1.5","2.3"]
["","النوع","","","","R-410A","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","م","20","20.0"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Sound power level","التبريد","","","dBA","63","66"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","825","900"]
["","","","العمق","mm","300","320"]
["","","","الارتفاع","mm","735","770"]
["الوزن","الوحدة","","","kg","47","71"]
["Power supply","الطور","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","","(2) - 220 فولت","(2) - 220 فولت"]
["","","","","","(3) - 230 فولت","(3) - 230 فولت"]
["","","","","","(4) - 240 فولت","(4) - 240 فولت"]