{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RKS-F"]
[]
[]
[]
[]
["","","","","","RKS60F3V1B","RKS71FAV1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","735","770"]
["","","","العرض","mm","825","900"]
["","","","العمق","mm","300","320"]
["الوزن","الوحدة","","","kg","47","71"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46"]
["Sound pressure level","Cooling","","High","dBA","49","52"]
["سائل تبريد","النوع","","","","R-410A","R-410A"]
["","السعة","","","kg","1.5","2.3"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","20","20.0"]
["Standard Accessories","دليل التركيب","","","","دليل التركيب","دليل التركيب"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]
["","","","","","(2) - 220 فولت","(2) - 220 فولت"]
["","","","","","(3) - 230 فولت","(3) - 230 فولت"]
["","","","","","(4) - 240 فولت","(4) - 240 فولت"]