{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RQ-BV3"]
[]
[]
[]
[]
["","","","","","RQ71B2V3B","RQ100B8V3B"]
["Sound pressure level","Cooling","","Nom.","dBA","50.0","53.0"]
["Standard Accessories","إعلان التوافق","","","","1","1"]
["","دليل التركيب","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","5.6","7.7"]
["","GWP","","","","2,087.5","2,087.5"]
["","Charge","","","kg","2.70","3.70"]
["","النوع","","","","R-410A","R-410A"]
["Operation range","Cooling","Ambient","Max.","درجة بمقياس الحوجلة الجافة","46.0","46.0"]
["","","","Min.","درجة بمقياس الحوجلة الجافة","-5.0","-5.0"]
["","Heating","Ambient","Max.","°مئوية مقياس الحوجلة الرطبة","15.0","15.0"]
["","","","Min.","°مئوية مقياس الحوجلة الرطبة","-10.0","-10.0"]
["Piping connections","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","70","70"]
["","","نظام","بدون شحن","م","30","30"]
["","","","مكافئ","م","90","90"]
["","Level difference","IU - IU","Max.","م","0.5","0.5"]
["","","IU - OU","Max.","م","30.0","30.0"]
["Sound power level","التبريد","","","dBA","63.0","66.0"]
["Dimensions","Unit","","العرض","mm","900","900"]
["","","","العمق","mm","320","320"]
["","","","الارتفاع","mm","770","1,170"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["الوزن","الوحدة","","","kg","84","103"]
["Power supply","الطور","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]