{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-J"]
[]
[]
[]
[]
["","","","","","RXG25J2V1B","RXG35J2V1B"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550"]
["","","","العرض","mm","765","765"]
["","","","العمق","mm","285","285"]
["الوزن","الوحدة","","","kg","34","34"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Sound pressure level","Cooling","","High","dBA","46","48"]
["","","","Low","dBA","43","44"]
["","Heating","","High","dBA","47","48"]
["","","","Low","dBA","44","45"]
["سائل تبريد","النوع","","","","R-410A","R-410A"]
["","السعة","","","kg","1.05","1.05"]
["","السعة","","","tCO2Eq","2.2","2.2"]
["","GWP","","","","2,087.5","2,087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","15","15"]
["Standard Accessories","دليل التركيب","","","","دليل التركيب","دليل التركيب"]
["","تجويف المصرف","","","","تجويف المصرف","تجويف المصرف"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة"]