{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":9,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-L"]
[]
[]
[]
[]
["","","","","","RXG20L2V1B","RXG25L2V1B","RXG35L2V1B","RXG50L2V1B"]
["Sound pressure level","Heating","","High","dBA","","47","48"]
["","Cooling","","High","dBA","","46","48"]
["Standard Accessories","وصلة (تصريف)","","","","","1","1"]
["","Installation manual","","","","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","","2.2","2.2"]
["","GWP","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","1.05","1.05"]
["","النوع","","","","","R-410A","R-410A"]
["Fan motor","Speed","Cooling","منخفض جداً","rpm","","780","780"]
["","","Heating","منخفض جداً","rpm","","740","740"]
["Piping connections","Level difference","IU - OU","Max.","م","","15","15"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Compressor","Type","","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","","765","765"]
["","","","العمق","mm","","285","285"]
["","","","الارتفاع","mm","","550","550"]
["الوزن","الوحدة","","","kg","","35","35"]
["Fan","Air flow rate","Heating","منخفض جداً","cfm","","932","932"]
["","","Cooling","منخفض جداً","cfm","","1,094","1,094"]
["Power supply","الطور","","","","","1~","1~"]
["","Frequency","","","Hz","","50","50"]
["","Voltage","","","V","","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 220 فولت","(2) - 220 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 230 فولت","(3) - 230 فولت","(3) - 240 فولت"]
["","","","","","(4) - نطاق التشغيلعند التركيب مع  Nexura، و FVXG-K، التبريد: الحد الأدنى 10°مئوية الحوجلة الجافة - الحد الأقصى 46°مئوية الحوجلة الجافة؛; التدفئة: الحد الأدنى -15°مئوية الحوجلة الرطبة - الحد الأقصى 18°مئوية الحوجلة الرطبة","(4) - 240 فولت","(4) - 240 فولت","(4) - نطاق التشغيلعند التركيب مع  Nexura، و FVXG-K، التبريد: الحد الأدنى 10°مئوية الحوجلة الجافة - الحد الأقصى 46°مئوية الحوجلة الجافة؛; التدفئة: الحد الأدنى -15°مئوية الحوجلة الرطبة - الحد الأقصى 18°مئوية الحوجلة الرطبة"]
["","","","","","","(5) - نطاق التشغيلعند التركيب مع  Nexura، و FVXG-K، التبريد: الحد الأدنى 10°مئوية الحوجلة الجافة - الحد الأقصى 46°مئوية الحوجلة الجافة؛; التدفئة: الحد الأدنى -15°مئوية الحوجلة الرطبة - الحد الأقصى 18°مئوية الحوجلة الرطبة","(5) - نطاق التشغيلعند التركيب مع  Nexura، و FVXG-K، التبريد: الحد الأدنى 10°مئوية الحوجلة الجافة - الحد الأقصى 46°مئوية الحوجلة الجافة؛; التدفئة: الحد الأدنى -15°مئوية الحوجلة الرطبة - الحد الأقصى 18°مئوية الحوجلة الرطبة"]
["","","","","","","(6) - يحتوي على غازات الاحتباس الحراري المفلورة","(6) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","31.0","","","42.6"]
["","","التدفئة","منخفض جداً","m³/min","26.4","","","38.3"]
["","","","منخفض جداً","cfm","1094","","","1504"]
["","","التدفئة","منخفض جداً","cfm","932","","","1352"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","","","735"]
["","","","العرض","mm","765","","","825"]
["","","","العمق","mm","285","","","300"]
["الوزن","الوحدة","","","kg","35","","","48"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","780","","","670"]
["","","التدفئة","منخفض جداً","rpm","740","","","670"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10 (5)","","","-10 (5)"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","","","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","","","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","","","18"]
["Sound pressure level","Cooling","","High","dBA","46","","","48"]
["","Heating","","High","dBA","47","","","48"]
["سائل تبريد","النوع","","","","R-410A","","","R-410A"]
["","السعة","","","kg","1.05","","","1.6"]
["","السعة","","","tCO2Eq","2.2","","","3.3"]
["","GWP","","","","2087.5","","","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","","","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","","","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","15","","","20"]
["Standard Accessories","Joint (drain)","","","","1","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","","","1~"]
["Power supply","Frequency","","","Hz","50","","","50"]
["","Voltage","","","V","220-240","","","220-240"]