{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-A9"]
[]
[]
[]
[]
["","","","","","RXJ20A5V1B9","RXJ25A5V1B9","RXJ35A5V1B9","RXJ42A5V1B9","RXJ50A5V1B9"]
["الأبعاد","الوحدة","","الارتفاع","mm","552","552","552","734","734"]
["","","","العرض","mm","840","840","840","954","954"]
["","","","العمق","mm","350","350","350","408","408"]
["الوزن","الوحدة","","","kg","32","32","32","49","49"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10","-10","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","50","50","50","50","50"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-21","-21","-21","-21","-21"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18","18","18","18"]
["Sound pressure level","Cooling","","Nom.","dBA","46","46","49","48","48"]
["","Heating","","Nom.","dBA","47","47","49","48","49"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32","R-32","R-32"]
["","السعة","","","kg","0.76","0.76","0.76","1.1","1.1"]
["","السعة","","","tCO2Eq","0.52","0.52","0.52","0.75","0.75"]
["","GWP","","","","675","675","675","675","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20","20","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","15","15","15","20","20"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1","1"]
["","Drain cap","","","","","","","3","3"]
["","Drain plug","","","","1","1","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة"]