{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":13,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-J"]
[]
[]
[]
[]
["","","","","","RXL20J2V1B","RXL25J2V1B","RXL35J2V1B","RXL35J3V1B","RXL42J2V1B","RXL42J3V1B","RXL50J2V1B","RXL50J3V1B"]
["Sound pressure level","Heating","","High","dBA","47","47","48","","48","","48"]
["","Cooling","","High","dBA","46","46","48","","48","","48"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","سدادة المصرف","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","1.7","2.1","2.5","","2.7","","3.5"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","","2,087.5","","2,087.5"]
["","Charge","","","kg","0.8","1.0","1.2","","1.3","","1.7"]
["","النوع","","","","R-410A","R-410A","R-410A","","R-410A","","R-410A"]
["Fan motor","Speed","Cooling","منخفض جداً","rpm","780","780","780","","790","","670"]
["","","Heating","منخفض جداً","rpm","740","740","740","","780","","670"]
["Piping connections","Level difference","IU - OU","Max.","م","15","15","15","","15","","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)"]
["Sound power level","التبريد","","","dBA","61","61","63","","63","","63"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","765","765","765","","765","","825"]
["","","","العمق","mm","285","285","285","","285","","300"]
["","","","الارتفاع","mm","550","550","550","","550","","735"]
["الوزن","الوحدة","","","kg","32","34","34","","39","","48"]
["Fan","Air flow rate","Heating","منخفض جداً","cfm","1,006","904","904","","960","","1,522"]
["","","Cooling","منخفض جداً","cfm","1,155","1,063","1,063","","1,080","","1,727"]
["Power supply","الطور","","","","1~","1~","1~","","1~","","1~"]
["","Frequency","","","Hz","50","50","50","","50","","50"]
["","Voltage","","","V","220-230-240","220-230-240","220-230-240","","220-240","","220-240"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","","","","30.1","","30.6","","48.9"]
["","","التدفئة","منخفض جداً","m³/min","","","","25.6","","27.2","","43.1"]
["","","","منخفض جداً","cfm","","","","1063","","1080","","1727"]
["","","التدفئة","منخفض جداً","cfm","","","","904","","960","","1522"]
["الأبعاد","الوحدة","","الارتفاع","mm","","","","550","","550","","735"]
["","","","العرض","mm","","","","765","","765","","825"]
["","","","العمق","mm","","","","285","","285","","300"]
["الوزن","الوحدة","","","kg","","","","34","","39","","48"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","","","","780","","790","","670"]
["","","التدفئة","منخفض جداً","rpm","","","","740","","780","","670"]
["Compressor","Type","","","","","","","ضاغط متأرجح محكم مانع للتسريب","","ضاغط متأرجح محكم مانع للتسريب","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","","","","-10","","-10","","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","","","","46","","46","","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","","","-25","","-25","","-25"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","","","18","","18","","18"]
["Sound pressure level","Cooling","","High","dBA","","","","48","","48","","48"]
["","Heating","","High","dBA","","","","48","","48","","48"]
["سائل تبريد","النوع","","","","","","","R-410A","","R-410A","","R-410A"]
["","السعة","","","kg","","","","1.2","","1.3","","1.7"]
["","السعة","","","tCO2Eq","","","","2.5","","2.7","","3.5"]
["","GWP","","","","","","","2087.5","","2087.5","","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","","","20","","20","","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","","","","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","","","","15","","15","","20"]
["وحدة التزويد بالطاقة","الطور","","","","","","","1~","","1~","","1~"]
["Power supply","Frequency","","","Hz","","","","50","","50","","50"]
["","Voltage","","","V","","","","220-240","","220-240","","220-240"]
["Notes","","","","","","","","(1) - 220 فولت","(1) - يتم تثبيت سخّان بدرج صرف في الوحدة الخارجية","(1) - 220 فولت","(1) - يتم تثبيت سخّان بدرج صرف في الوحدة الخارجية","(1) - 220 فولت"]
["","","","","","","","","(2) - 230 فولت","(2) - 220 فولت","(2) - 230 فولت","(2) - 220 فولت","(2) - 230 فولت"]
["","","","","","","","","(3) - 240 فولت","(3) - 230 فولت","(3) - 240 فولت","(3) - 230 فولت","(3) - 240 فولت"]
["","","","","","","","","","(4) - 240 فولت","","(4) - 240 فولت"]
["","","","","","","","","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة"]