{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","","","30.1","30.6","48.9"]
["","","التدفئة","منخفض جداً","m³/min","","","25.6","27.2","43.1"]
["","","","منخفض جداً","cfm","","","1063","1080","1727"]
["","","التدفئة","منخفض جداً","cfm","","","904","960","1522"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550","550","550","735"]
["","","","العرض","mm","765","765","765","765","825"]
["","","","العمق","mm","285","285","285","285","300"]
["الوزن","الوحدة","","","kg","34","34","34","39","47"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","780","780","780","790","670"]
["","","التدفئة","منخفض جداً","rpm","740","740","740","780","670"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10","-10","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46","46","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-25","-25","-25","-25","-25"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18","18","18","18"]
["Sound pressure level","Cooling","","High","dBA","46","46","48","48","48"]
["","Heating","","High","dBA","47","47","48","48","48"]
["سائل تبريد","النوع","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","السعة","","","kg","1.0","1.05","1.2","1.3","1.7"]
["","السعة","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20","20","20","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","15","15","15","15","20"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1","1"]
["","سدادة المصرف","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Notes","","","","","(1) - يتم تثبيت سخّان بدرج صرف في الوحدة الخارجية","(1) - يتم تثبيت سخّان بدرج صرف في الوحدة الخارجية","(1) - يتم تثبيت سخّان بدرج صرف في الوحدة الخارجية","(1) - يتم تثبيت سخّان بدرج صرف في الوحدة الخارجية","(1) - يتم تثبيت سخّان بدرج صرف في الوحدة الخارجية"]
["","","","","","(2) - 220 فولت","(2) - 220 فولت","(2) - 220 فولت","(2) - 220 فولت","(2) - 220 فولت"]
["","","","","","(3) - 230 فولت","(3) - 230 فولت","(3) - 230 فولت","(3) - 230 فولت","(3) - 230 فولت"]
["","","","","","(4) - 240 فولت","(4) - 240 فولت","(4) - 240 فولت","(4) - 240 فولت","(4) - 240 فولت"]
["","","","","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","(5) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(5) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(5) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]
["","","","","","","","(6) - يحتوي على غازات الاحتباس الحراري المفلورة","(6) - يحتوي على غازات الاحتباس الحراري المفلورة","(6) - يحتوي على غازات الاحتباس الحراري المفلورة"]