{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","30.6","30.6"]
["","","التدفئة","منخفض جداً","m³/min","27.2","27.2"]
["","","","منخفض جداً","cfm","1080","1080"]
["","","التدفئة","منخفض جداً","cfm","960","960"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550"]
["","","","العرض","mm","858","858"]
["","","","العمق","mm","330","330"]
["الوزن","الوحدة","","","kg","40","40"]
["Compressor","Type","","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-25","-25"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18","18"]
["Sound pressure level","Cooling","","High","dBA","48","48"]
["","","","Low","dBA","44","44"]
["","Heating","","High","dBA","49","49"]
["","","","Low","dBA","45","45"]
["سائل تبريد","النوع","","","","R-410A","R-410A"]
["","السعة","","","kg","1","1"]
["","السعة","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20","20"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - IU","Max.","م","15","15"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب"]