{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A8"]
[]
[]
[]
[]
["","","","","","RXM50A5V1B8"]
["الأبعاد","الوحدة","","الارتفاع","mm","610"]
["","","","العرض","mm","923"]
["","","","العمق","mm","367"]
["الوزن","الوحدة","","","kg","40"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","600"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","50 (1), 46 (1)"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-21 (1), -15 (1)"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18"]
["Sound pressure level","Cooling","","Nom.","dBA","48"]
["","Heating","","Nom.","dBA","49"]
["سائل تبريد","النوع","","","","R-32"]
["","السعة","","","kg","0.95"]
["","السعة","","","tCO2Eq","0.65"]
["","GWP","","","","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","20"]
["Standard Accessories","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["وحدة التزويد بالطاقة","الطور","","","","1~"]
["Power supply","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","(3) - يحتوي على غازات الاحتباس الحراري المفلورة"]