{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["المروحة","معدل تدفق الهواء","التبريد","منخفض جداً","m³/min","46.0"]
["","","التدفئة","منخفض جداً","m³/min","46.0"]
["","","","منخفض جداً","cfm","1624"]
["","","التدفئة","منخفض جداً","cfm","1624"]
["الأبعاد","الوحدة","","الارتفاع","mm","770"]
["","","","العرض","mm","900"]
["","","","العمق","mm","320"]
["الوزن","الوحدة","","","kg","71"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","730"]
["","","التدفئة","منخفض جداً","rpm","730"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18"]
["Sound pressure level","Cooling","","High","dBA","52"]
["","Heating","","High","dBA","52"]
["سائل تبريد","النوع","","","","R-410A"]
["","السعة","","","kg","2.3"]
["","السعة","","","tCO2Eq","4.8"]
["","GWP","","","","2,087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","20"]
["Standard Accessories","دليل التركيب","","","","1"]
["","ملصق الشحن بسائل التبريد","","","","1"]
["","ملصقات متعددة اللغات حول غازات الدفيئة المفلورة","","","","1"]
["","مأخذ تصريف","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~"]
["Power supply","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]
["","","","","","(2) - 220 فولت"]
["","","","","","(3) - 230 فولت"]
["","","","","","(4) - 240 فولت"]
["","","","","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة"]