{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B","RXTP35N2V1B"]
["Sound pressure level","Heating","","Nom.","dBA","49"]
["","Cooling","","Nom.","dBA","48"]
["Standard Accessories","دليل التركيب","","","","1"]
["","ملصق الشحن بسائل التبريد","","","","1","1"]
["","ملصقات متعددة اللغات حول غازات الدفيئة المفلورة","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","","Expansion valve (electronic type)"]
["","GWP","","","","675"]
["","Charge","","","kg","1.1"]
["","النوع","","","","R-32","1.1"]
["Fan motor","Speed","Cooling","منخفض جداً","rpm","450"]
["","","Heating","منخفض جداً","rpm","360"]
["Operation range","Cooling","Ambient","Max.","درجة بمقياس الحوجلة الجافة","46"]
["","","","Min.","درجة بمقياس الحوجلة الجافة","-10"]
["","Heating","Ambient","Max.","°مئوية مقياس الحوجلة الرطبة","18"]
["","","","Min.","°مئوية مقياس الحوجلة الرطبة","-25"]
["Piping connections","Level difference","IU - OU","Max.","م","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","763","650"]
["","","","العمق","mm","312","920"]
["","","","الارتفاع","mm","551","312"]
["الوزن","الوحدة","","","kg","38","38"]
["Power supply","الطور","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["","","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["Sound pressure level","Heating","","High","dBA","","49"]
["Standard Accessories","551","","","","","763"]
["Fan motor","Speed","Cooling","منخفض جداً","rpm","","360"]
["","","Heating","منخفض جداً","rpm","","-25"]
["Sound pressure level","Cooling","","High","dBA","","48"]