{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N9"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B9","RXTP35N2V1B9"]
["Sound pressure level","Heating","","Nom.","dBA","49","49"]
["","Cooling","","Nom.","dBA","48","48"]
["Standard Accessories","دليل التركيب","","","","1","1"]
["","ملصق الشحن بسائل التبريد","","","","1","1"]
["","ملصقات متعددة اللغات حول غازات الدفيئة المفلورة","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["","Charge","","","kg","1.1","1.1"]
["","النوع","","","","R-32","R-32"]
["Fan motor","Speed","Cooling","منخفض جداً","rpm","450","450"]
["","","Heating","منخفض جداً","rpm","360","360"]
["Operation range","Cooling","Ambient","Max.","درجة بمقياس الحوجلة الجافة","46","46"]
["","","","Min.","درجة بمقياس الحوجلة الجافة","-10","-10"]
["","Heating","Ambient","Max.","°مئوية مقياس الحوجلة الرطبة","18","18"]
["","","","Min.","°مئوية مقياس الحوجلة الرطبة","-25","-25"]
["Piping connections","Level difference","IU - OU","Max.","م","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","763","763"]
["","","","العمق","mm","312","312"]
["","","","الارتفاع","mm","551","551"]
["الوزن","الوحدة","","","kg","38","38"]
["Power supply","الطور","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["","","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]