{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Dimensions","Unit","","الارتفاع","mm","870","870"]
["","","","العرض","mm","1,100","1,100"]
["","","","العمق","mm","460","460"]
["الوزن","الوحدة","","","kg","117","117"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-20","-20"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-20","-20"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","15","15"]
["Sound power level","التبريد","","","dBA","73","76"]
["","التدفئة","","","dBA","76 (1)","79 (1)"]
["Sound pressure level","Cooling","","Nom.","dBA","53","57"]
["","Heating","","Nom.","dBA","60","63"]
["Refrigerant","النوع","","","","R-32","R-32"]
["","Charge","","","kg","5","5"]
["","GWP","","","","675","675"]
["Piping connections","Liquid","","القطر الخارجي","mm","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","22.2","22.2"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","100","100"]
["","","نظام","بدون شحن","م","30","30"]
["","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual"]
["Standard Accessories","دليل التركيب","","","","1","1"]
["","تدابير السلامة الوقائية العامة","","","","1","1"]
["","أغلفة برباط","","","","2","2"]
["","انزع ملصق الغاز F","","","","1","1"]
["","أنابيب توصيل","","","","6","6"]
["Power supply","الطور","","","","3~","3~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","380-415","380-415"]
["Current - 50Hz","قيمة الأمبير القصوى للفاصمة (MFA)","","","A","20","20"]
["Notes","","","","","(1) - حسب ENER Lot 21","(1) - حسب ENER Lot 21"]