{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-B9W1"]
[]
[]
[]
[]
["","","","","","RZQ100B9W1B","RZQ125B9W1B","RZQ140B9W1B"]
["Sound pressure level","Heating","","Nom.","dBA","51.0","52.0","52.0"]
["","Cooling","","Nom.","dBA","49.0","50.0","50.0"]
["Standard Accessories","أغلفة برباط","","","","2","2","2"]
["","Installation manual","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","9","9","9"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","4.30","4.30","4.30"]
["","النوع","","","","R-410A","R-410A","R-410A"]
["Piping connections","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","75","75","75"]
["","","نظام","بدون شحن","م","30","30","30"]
["","","","مكافئ","م","95","95","95"]
["","Level difference","IU - IU","Max.","م","0.5","0.5","0.5"]
["","","IU - OU","Max.","م","30.0","30.0","30.0"]
["","Additional refrigerant charge","","","kg/m","See installation manual 4PW21412-1","See installation manual 4PW21412-1","See installation manual 4PW21412-1"]
["Sound power level","التبريد","","","dBA","65.0","66.0","66.0"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Dimensions","Unit","","العرض","mm","900","900","900"]
["","","","العمق","mm","320","320","320"]
["","","","الارتفاع","mm","1,345","1,345","1,345"]
["الوزن","الوحدة","","","kg","106","106","106"]
["Power supply","الطور","","","","3N~","3N~","3N~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","400","400","400"]
["Notes","","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","","(2) - Power supply intake for FDQ: outdoor unit + indoor unit","(2) - Power supply intake for FDQ: outdoor unit + indoor unit","(2) - Power supply intake for FDQ: outdoor unit + indoor unit"]
["","","","","","(3) - 230 فولت","(3) - 230 فولت","(3) - 230 فولت"]
["","","","","","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة"]