{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Dimensions","Unit","","الارتفاع","mm","1,680"]
["","","","العرض","mm","930"]
["","","","العمق","mm","765"]
["الوزن","الوحدة","","","kg","183.0"]
["Compressor","Type","","","","Hermetically sealed scroll compressor"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-5.0"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46.0"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15.0"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","15.0"]
["Sound power level","التبريد","","","dBA","78.0"]
["","التدفئة","","","dBA","78.0"]
["Refrigerant","النوع","","","","R-410A"]
["","Charge","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Piping connections","Liquid","","القطر الخارجي","mm","9.52"]
["","غاز","","القطر الخارجي","mm","22.2"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","100"]
["","","نظام","بدون شحن","م","30"]
["Standard Accessories","دليل التركيب","","","","1"]
["","أنابيب توصيل","","","","4"]
["Power supply","الطور","","","","3N~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","380-415"]
["Current - 50Hz","قيمة الأمبير القصوى للفاصمة (MFA)","","","A","25"]
["Notes","","","","","(1) - وحدة التغذية للوحدة الداخلية FDQ منفصلة"]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["الأبعاد","الوحدة","","الارتفاع","mm","","1680"]
["","","","العرض","mm","","930"]
["","","","العمق","mm","","765"]
["الوزن","الوحدة","","","kg","","184.0"]
["ضاغط","نوع","","","","","ضاغط مخروطي محكم ضد التسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","","-5.0"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","","46.0"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","-15.0"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","15.0"]
["مستوى طاقة الصوت","التبريد","","","dBA","","78.0"]
["","التدفئة","","","dBA","","78.0"]
["سائل تبريد","السعة","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","السعة","","","tCO2Eq","","19.4"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","","12.70"]
["","غاز","","القطر الخارجي","mm","","22.2"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","100"]
["","","نظام","بدون شحن","م","","30"]
["Standard Accessories","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Power supply","Frequency","","","Hz","","50"]
["تيار - 50 هرتز","قيمة الأمبير القصوى للفاصمة (MFA)","","","A","","25"]