{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":9,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQG-L"]
[]
[]
[]
[]
["","","","","","RZQG71LV1B","RZQG100LV1B","RZQG125LV1B","RZQG140LV1B"]
["Sound pressure level","Heating","","Nom.","dBA","","","53"]
["","Cooling","","Nom.","dBA","","","51"]
["Refrigerant","Charge","","","TCO2Eq","","","8.4"]
["","GWP","","","","","","2,087.5"]
["","Charge","","","kg","","","4.0"]
["","النوع","","","","","","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","م","","","30"]
["Sound power level","التبريد","","","dBA","","","67"]
["Compressor","Type","","","","","","Hermetically sealed rotary compressor"]
["Dimensions","Unit","","العرض","mm","","","940"]
["","","","العمق","mm","","","320"]
["","","","الارتفاع","mm","","","1,430"]
["الوزن","الوحدة","","","kg","","","99"]
["Power supply","الطور","","","","","","1~"]
["","Frequency","","","Hz","","","50"]
["","Voltage","","","V","","","220-240"]
["Notes","","","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["الأبعاد","الوحدة","","الارتفاع","mm","990","1430","","1430"]
["","","","العرض","mm","940","940","","940"]
["","","","العمق","mm","320","320","","320"]
["الوزن","الوحدة","","","kg","77","99","","99"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-15","-15","","-15"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","50","50","","50"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-20","-20","","-20"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","15.5","15.5","","15.5"]
["Sound pressure level","Cooling","","Nom.","dBA","48","50","","51"]
["","Heating","","Nom.","dBA","50","52","","53"]
["سائل تبريد","السعة","","","kg","3.5","4.0","","4.0"]
["","السعة","","","tCO2Eq","7.3","8.4","","8.4"]
["","GWP","","","","2087.5","2087.5","","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","50","75","","75"]
["Piping connections","Level difference","IU - OU","Max.","م","30","30","","30"]
["Power supply","Frequency","","","Hz","50","50","","50"]