{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQG-L8/7V1"]
[]
[]
[]
[]
["","","","","","RZQG71L8V1B","RZQG100L8V1B","RZQG125L8V1B","RZQG140L7V1B"]
["مستوى طاقة الصوت","التبريد","","","dBA","64","66","67","69"]
["الأبعاد","الوحدة","","الارتفاع","mm","990","1430","1430","1430"]
["","","","العرض","mm","940","940","940","940"]
["","","","العمق","mm","320","320","320","320"]
["الوزن","الوحدة","","","kg","78","102","102","102"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-15","-15","-15","-15"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","50","50","50","50"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-20","-20","-20","-20"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","15.5","15.5","15.5","15.5"]
["Sound pressure level","Cooling","","Nom.","dBA","48","50","51","52"]
["","Heating","","Nom.","dBA","50","52","53","53"]
["","Night quiet mode","","Level 1","dBA","43","45","45","45"]
["سائل تبريد","النوع","","","","R-410A","R-410A","R-410A","R-410A"]
["","السعة","","","kg","2.9","4.0","4.0","4.0"]
["","السعة","","","tCO2Eq","6.1","8.4","8.4","8.4"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","50","75","75","75"]
["Piping connections","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual","See installation manual","See installation manual"]
["","Level difference","IU - OU","Max.","م","30.0","30.0","30.0","30.0"]
["","","IU - IU","Max.","م","0.5","0.5","0.5","0.5"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(4) - 3 مع إعادة الشحن","(4) - 3 مع إعادة الشحن","(4) - 3 مع إعادة الشحن","(4) - 3 مع إعادة الشحن"]