{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":9,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQG-LY1L"]
[]
[]
[]
[]
["","","","","","RZQG71L8Y1L","RZQG100L8Y1L","RZQG125L8Y1L","RZQG140L7Y1L"]
["Sound pressure level","Heating","","Nom.","dBA","50","52","53","53"]
["","Cooling","","Nom.","dBA","48","50","51","52"]
["Standard Accessories","أغلفة برباط","","","","2","2","2","2"]
["","دليل التركيب","","","","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","6.10","8.40","8.40","8.40"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","2.9","4.0","4.0","4.0"]
["","النوع","","","","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Liquid","","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","50","75","75","75"]
["","","نظام","بدون شحن","م","30","30","30","30"]
["","","","مكافئ","م","70","90","90","90"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9","15.9"]
["","Level difference","IU - IU","Max.","م","0.5","0.5","0.5","0.5"]
["","","IU - OU","Max.","م","30.0","30.0","30.0","30.0"]
["","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual","See installation manual","See installation manual"]
["Sound power level","التبريد","","","dBA","64","66","67","69"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","940","940","940","940"]
["","","","العمق","mm","320","320","320","320"]
["","","","الارتفاع","mm","990","1,430","1,430","1,430"]
["الوزن","الوحدة","","","kg","80","101","101","101"]
["Power supply","الطور","","","","3N~","3N~","3N~","3N~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415","380-415"]
["Notes","","","","","(1) - 3 مع إعادة الشحن","(1) - 3 مع إعادة الشحن","(1) - 3 مع إعادة الشحن","(1) - 3 مع إعادة الشحن"]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","(3) - PED: التجميع = الفئة l : مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(3) - PED: التجميع = الفئة l : مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(3) - PED: التجميع = الفئة l : مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(3) - PED: التجميع = الفئة l : مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC"]