{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":10,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","","RZQSG71L2V1B","RZQSG100L7V1B","RZQSG100L7Y1B9","RZQSG125L7Y1B9","RZQSG125L7V1B"]
["Sound pressure level","Heating","","Nom.","dBA","","","","58"]
["","Cooling","","Nom.","dBA","","","","54"]
["Standard Accessories","أغلفة برباط","","","","","","","2"]
["","دليل التركيب","","","","","","","1"]
["Refrigerant","Charge","","","TCO2Eq","","","","6.1"]
["","GWP","","","","","","","2,087.5"]
["","Charge","","","kg","","","","2.9"]
["","النوع","","","","","","","R-410A"]
["Operation range","Cooling","Ambient","Max.","درجة بمقياس الحوجلة الجافة","","","","46.0"]
["","","","Min.","درجة بمقياس الحوجلة الجافة","","","","-5.0"]
["","Heating","Ambient","Max.","°مئوية مقياس الحوجلة الرطبة","","","","15.5"]
["","","","Min.","°مئوية مقياس الحوجلة الرطبة","","","","-15.0"]
["Piping connections","Liquid","","القطر الخارجي","mm","","","","9.52"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","","","50"]
["","","نظام","بدون شحن","م","","","","30"]
["","","","مكافئ","م","","","","70"]
["","غاز","","القطر الخارجي","mm","","","","15.9"]
["","Level difference","IU - IU","Max.","م","","","","0.5"]
["","","IU - OU","Max.","م","","","","30.0"]
["","Additional refrigerant charge","","","kg/m","","","","انظر دليل التركيب 4P302555-1"]
["Sound power level","التبريد","","","dBA","","","","70"]
["Compressor","Type","","","","","","","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","","","","940"]
["","","","العمق","mm","","","","320"]
["","","","الارتفاع","mm","","","","990"]
["الوزن","الوحدة","","","kg","","","","82"]
["Power supply","الطور","","","","","","","3N~"]
["","Frequency","","","Hz","","","","50"]
["","Voltage","","","V","","","","380-415"]
["Notes","","","","","","","","(1) - PED: التجميع = الفئة l : مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC"]
["","","","","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","","","","(3) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["الأبعاد","الوحدة","","الارتفاع","mm","770","990","990","","990"]
["","","","العرض","mm","900","940","940","","940"]
["","","","العمق","mm","320","320","320","","320"]
["الوزن","الوحدة","","","kg","67","81","82","","81"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","-5.0","-5.0","-5.0","","-5.0"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46","46.0","46.0","","46.0"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15.0","-15.0","","-15.0"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","15.5","15.5","15.5","","15.5"]
["مستوى طاقة الصوت","التبريد","","","dBA","65","69","69","","70"]
["Sound pressure level","Cooling","","Nom.","dBA","49","53","53","","54"]
["","Heating","","Nom.","dBA","51","57","57","","58"]
["سائل تبريد","السعة","","","kg","2.75","2.9","2.9","","2.9"]
["","GWP","","","","2087.5","2087.5","2087.5","","2087.5"]
["","السعة","","","tCO2Eq","5.7","6.1","6.1","","6.1"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52","","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9","","15.9"]
["","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","30","50","50","","50"]
["","","نظام","مكافئ","م","40","70","70","","70"]
["","","","بدون شحن","م","30","30","30","","30"]
["Piping connections","Level difference","IU - OU","Max.","م","15","30.0","30.0","","30.0"]
["","","IU - IU","Max.","م","0.5","0.5","0.5","","0.5"]
["Standard Accessories","Installation manual","","","","1","1","1","","1"]
["","Tie-wraps","","","","2","2","2","","2"]
["Power supply","Frequency","","","Hz","50","50","50","","50"]
["تيار - 50 هرتز","قيمة الأمبير القصوى للفاصمة (MFA)","","","A","20","32","20","","32"]
["Sound pressure level","Night quiet mode","","Level 1","dBA","","","49"]