{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RZAG-B"]
[]
[]
[]
[]
["","","","","FNA35A2VEB9 / RZAG35B5V1B","FNA60A2VEB9 / RZAG50B5V1B","FNA50A2VEB9 / RZAG50B5V1B","FNA60A2VEB9 / RZAG60B5V1B"]
["Cooling capacity","Min.","","kW","1.6","1.7","1.7","1.7"]
["","Nom.","","kW","3.5","5","5","6"]
["","Max.","","kW","4.5","6","6","6.5"]
["Heating capacity","Min.","","kW","1.4","1.7","1.7","1.7"]
["","Nom.","","kW","4","5","5","7"]
["","Max.","","kW","5","6","6","7.5"]
["Nominal efficiency","EER","","","3.9","3.98","3.8","3.4"]
["","COP","","","3.5","3.44","3.4","3.3"]
["","Annual energy consumption","","kWh","449","628","658","882"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","B","B","C","C"]
["Space cooling","Energy efficiency class","","","A+","A+","A+","A+"]
["","Capacity","Pdesign","kW","3.5","5","5","6"]
["","SEER","","","5.9","5.98","5.9","5.7"]
["","Annual energy consumption","","kWh/a","208","293","297","368"]
["Space heating (Average climate)","Energy efficiency class","","","A","A","A","A"]
["","Capacity","Pdesign","kW","3.5","4.3","4.3","4.5"]
["","SCOP/A","","","3.9","3.94","3.9","3.9"]
["","Pdh Heating capacity at -10°","","kW","2.99","3.63","3.62","3.82"]
["","Annual energy consumption","","kWh/a","1255","1528","1542","1616"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]