{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":14,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / RXJ-M"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / RXJ20M2V1B","FTXJ20MV1BW / RXJ20M3V1B","FTXJ20MV1BW / RXJ20M5V1B","FTXJ25MV1BW / RXJ25M2V1B","FTXJ25MV1BW / RXJ25M3V1B","FTXJ25MV1BW / RXJ25M5V1B","FTXJ35MV1BW / RXJ35M2V1B","FTXJ35MV1BW / RXJ35M5V1B","FTXJ35MV1BW / RXJ35M3V1B","FTXJ50MV1BW / RXJ50MV1B"]
["Cooling capacity","Min.","","kW","","1.30","","","0.90"]
["","Max.","","kW","","2.80","","","3.30"]
["","Nom.","","kW","2.3","2.30","2.30","2.4","2.40","2.40","3.5","3.50","","4.80"]
["Space cooling","SEER","","","8.73","8.73","8.73","8.64","8.64","8.64","7.19","7.19","","7.02"]
["","Annual energy consumption","","kWh/a","92","92","92","97","97","97","170","170","","239"]
["","Capacity","Pdesign","kW","2.30","2.30","2.3","2.40","2.40","2.4","3.50","3.5","","4.80"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++","A++","A++","","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.10","2.10","2.10","2.70","2.70","2.70","3.00","3.00","","4.60"]
["","SCOP/A","","","4.61","4.60","4.61","4.60","4.60","4.60","4.60","4.60","","4.28"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","","A+"]
["","Pdh Heating capacity at -10°","","kW","1.80","1.80","1.80","2.18","2.18","2.18","2.61","2.61","","4.16"]
["","Annual energy consumption","","kWh/a","638","639","638","822","821","822","913","913","","1,505"]
["Nominal efficiency","Annual energy consumption","","kWh","248","248","248","254","254","254","428","428","","716"]
["","EER","","","4.64","4.64","4.64","4.73","4.73","4.73","4.09","4.09","","3.35"]
["","COP","","","5.00","5.00","5.00","4.57","4.57","4.57","4.04","4.04","","3.65"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","","A"]
["","","Heating","","A","A","A","A","A","A","A","A","","A"]
["Heating capacity","Nom.","","kW","2.5","2.50","2.5","3.2","3.20","3.2","4","4.0","","5.80"]
["","Min.","","kW","","1.30","","","0.90"]
["","Max.","","kW","","4.30","","","4.70"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["Cooling capacity","Min.","","kW","","","","","","","","","0.90"]
["","Nom.","","kW","","","","","","","","","3.50"]
["","Max.","","kW","","","","","","","","","4.10"]
["Heating capacity","Min.","","kW","","","","","","","","","0.90"]
["","Nom.","","kW","","","","","","","","","4.00"]
["","Max.","","kW","","","","","","","","","5.10"]
["Nominal efficiency","EER","","","","","","","","","","","4.09"]
["","COP","","","","","","","","","","","4.04"]
["","Annual energy consumption","","kWh","","","","","","","","","428"]
["","Energy labeling Directive","Cooling","","","","","","","","","","A"]
["","","Heating","","","","","","","","","","A"]
["Space cooling","Energy efficiency class","","","","","","","","","","","A++"]
["","Capacity","Pdesign","kW","","","","","","","","","3.50"]
["","SEER","","","","","","","","","","","7.19"]
["","Annual energy consumption","","kWh/a","","","","","","","","","170"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","","","","A++"]
["","Capacity","Pdesign","kW","","","","","","","","","3.00"]
["","SCOP/A","","","","","","","","","","","4.60"]
["","Pdh Heating capacity at -10°","","kW","","","","","","","","","2.61"]
["","Annual energy consumption","","kWh/a","","","","","","","","","913"]