{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":10,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N / RXZ-N"]
[]
[]
[]
[]
["","","","","FTXZ25NV1B / RXZ25NV1B","FTXZ25NV1B / RXZ25NV1B9","FTXZ35NV1B / RXZ35NV1B","FTXZ35NV1B / RXZ35NV1B9","FTXZ50NV1B / RXZ50NV1B9","FTXZ50NV1B / RXZ50NV1B"]
["Cooling capacity","Min.","","kW","0.6","0.6","0.6","0.6","0.6"]
["","Max.","","kW","3.9","3.9","5.3","5.3","5.8"]
["","Nom.","","kW","2.5","2.5","3.5","3.5","5.0"]
["Space cooling","SEER","","","9.54","9.54","9.00","9.00","8.60"]
["","Annual energy consumption","","kWh/a","92","92","136","136","203"]
["","Capacity","Pdesign","kW","2.50","2.50","3.50","3.50","5.00"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.50","3.50","4.50","4.50","5.60"]
["","SCOP/A","","","5.90","5.90","5.73","5.73","5.50"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++"]
["","Annual energy consumption","","kWh/a","831","831","1,100","1,100","1,427"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5","9.5"]
["Nominal efficiency","Annual energy consumption","","kWh","205","205","330","330","550"]
["","EER","","","6.10","6.10","5.30","5.30","4.55"]
["","COP","","","5.80","5.80","5.00","5.00","4.47"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.6","3.6","5.0","5.0","6.3"]
["","Min.","","kW","0.6","0.6","0.6","0.6","0.6"]
["","Max.","","kW","7.5","7.5","9.0","9.0","9.4"]
["Notes","","","","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(1) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(1) - 230V"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 240V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]
["Cooling capacity","Min.","","kW","","","","","","0.6"]
["","Nom.","","kW","","","","","","5.0"]
["","Max.","","kW","","","","","","5.8"]
["Heating capacity","Min.","","kW","","","","","","0.6"]
["","Nom.","","kW","","","","","","6.3"]
["","Max.","","kW","","","","","","9.4"]
["Nominal efficiency","EER","","","","","","","","4.55"]
["","COP","","","","","","","","4.47"]
["","Annual energy consumption","","kWh","","","","","","550"]
["","Energy labeling Directive","Cooling","","","","","","","A"]
["","","Heating","","","","","","","A"]
["Piping connections","Gas","OD","mm","","","","","","9.5"]
["","Liquid","OD","mm","","","","","","6.35"]
["Space cooling","Energy efficiency class","","","","","","","","A+++"]
["","Capacity","Pdesign","kW","","","","","","5.00"]
["","SEER","","","","","","","","8.60"]
["","Annual energy consumption","","kWh/a","","","","","","203"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","A+++"]
["","Capacity","Pdesign","kW","","","","","","5.60"]
["","SCOP/A","","","","","","","","5.50"]
["","Annual energy consumption","","kWh/a","","","","","","1427"]