{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":9,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWR-AF"]
[]
[]
[]
[]
["","","","","","FWR02AAFV3","FWR03AAFV3","FWR06AAFV3","FWR08AAFV3"]
["Sound pressure level","Low","","","dBA","33 (6)","28 (6)","43 (6)","43 (5)"]
["","High","","","dBA","45 (6)","42 (6)","54 (6)","61 (5)"]
["Total sound power level","Low","","","dBA","38 (4)","33 (4)","48 (4)","48 (4)"]
["","High","","","dBA","50 (4)","47 (4)","58 (4)","66 (4)"]
["Water flow","Cooling","","Low","l/h","216 (1)","297 (1)","535 (1)","699 (1)"]
["","","","High","l/h","307 (1)","493 (1)","802 (1)","1,352 (1)"]
["","Heating","","High","l/h","154 (3)","234 (3)","406 (3)","643 (3)"]
["","","","Low","l/h","119 (3)","165 (3)","311 (3)","425 (3)"]
["","Water pressure drop","Heating","High","kPa","6 (3)","4 (3)","8 (3)","29 (3)"]
["","","","Low","kPa","5 (3)","2 (3)","5 (3)","14 (3)"]
["","","Cooling","High","kPa","13 (1)","11 (1)","14 (1)","16 (1)"]
["","","","Low","kPa","7 (1)","5 (1)","7 (1)","5 (1)"]
["Piping connections","Drain","","OD","mm","16","16","16","16"]
["Power input","High","","","kW","0.019","0.016","0.033","0.087"]
["","Low","","","kW","0.01","0.01","0.01","0.013"]
["Allowed water temperature","Heating","","Max.","°C","95.000","95.000","95.000","95.000"]
["","","","Min.","°C","5.00","5.00","5.00","5.00"]
["","Cooling","","Min.","°C","5","5","5","5"]
["","","","Max.","°C","95.0","95.0","95.0","95.0"]
["Dimensions","Unit","","Width","mm","774","984","1,190","1,404"]
["","","","Depth","mm","246","246","246","271"]
["","","","Height","mm","564","564","564","564"]
["Water connections","Additional coil","","","inch","1/2\"","1/2\"","1/2\"","1/2\""]
["","Primary coil","","","inch","1/2\"","1/2\"","1/2\"","3/4 \""]
["Casing","Colour","","","","White - RAL9010","White - RAL9010","White - RAL9010"]
["Weight","Unit","","","kg","21.2","27.5","33.6","43.1"]
["Fan","Air flow rate","","Low","m³/h","205","237","460","636"]
["","","","High","m³/h","327","431","763","1,362"]
["Cooling capacity (standard conditions)","Total capacity 4-pipe","","Low","kW","1.25 (1)","1.72 (1)","3.10 (1)","4.06 (1)"]
["","","","High","kW","1.77 (1)","2.86 (1)","4.64 (1)","7.79 (1)"]
["","Sensible capacity 4-pipe","","Low","kW","0.97 (1)","1.23 (1)","2.27 (1)","3.01 (1)"]
["","","","High","kW","1.44 (1)","2.06 (1)","3.54 (1)","5.76 (1)"]
["Heating capacity (standard conditions)","Capacity 4-pipe","","Low","kW","1.36 (3)","1.88 (3)","3.55 (3)","4.85 (3)"]
["","","","High","kW","1.76 (3)","2.68 (3)","4.64 (3)","7.35 (3)"]
["Power supply","Type","","","","230 /  1 /  50","230 /  1 /  50","230 /  1 /  50","230 /  1 /  50"]
["","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","230","230","230","230"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K."]
["","","","","","(2) - Heating: indoor temp. 20°CDB, 15°CWB; entering water temp. 45°C, water temperature drop 5K.","(2) - Heating: indoor temp. 20°CDB, 15°CWB; entering water temp. 45°C, water temperature drop 5K.","(2) - Heating: indoor temp. 20°CDB, 15°CWB; entering water temp. 45°C, water temperature drop 5K.","(2) - Heating: indoor temp. 20°CDB, 15°CWB; entering water temp. 45°C, water temperature drop 5K."]
["","","","","","(3) - Heating: indoor temp. 20°CDB, 15°CWB; entering water temp. 65°C, water temperature drop 10K.","(3) - Heating: indoor temp. 20°CDB, 15°CWB; entering water temp. 65°C, water temperature drop 10K.","(3) - Heating: indoor temp. 20°CDB, 15°CWB; entering water temp. 65°C, water temperature drop 10K.","(3) - Heating: indoor temp. 20°CDB, 15°CWB; entering water temp. 65°C, water temperature drop 10K."]
["","","","","","(4) - Sound power level according to ISO3741","(4) - Sound power level according to ISO3741","(4) - Sound power level according to ISO3741","(4) - Sound power level according to ISO3741"]
["","","","","","(5) - SL: The silent fan level of the air flow rate setting","(5) - SL: The silent fan level of the air flow rate setting","(5) - SL: The silent fan level of the air flow rate setting","(5) - The sound pressure level is measured via a microphone at 1m distance of the unit."]
["","","","","","(6) - The sound pressure level is measured via a microphone at 1m distance of the unit.","(6) - The sound pressure level is measured via a microphone at 1m distance of the unit.","(6) - The sound pressure level is measured via a microphone at 1m distance of the unit."]