{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":9,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","برغي+حلقة","","","","برغي+حلقة"]
["","جهاز تحكم عن بعد لاسلكي","","","","جهاز تحكم عن بعد لاسلكي"]
["","مشوى بغطاء مع قفل","","","","مشوى بغطاء مع قفل"]
["","بطارية","","","","بطارية"]
["Piping connections","Liquid","","القطر الخارجي","mm","9.52"]
["","غاز","","القطر الخارجي","mm","15.88"]
["","Drain","","","","19.05"]
["Power input","Cooling","","Nom.","kW","0.128"]
["","Heating","","Nom.","kW","0.128"]
["Sound power level","التبريد","","","dBA","64"]
["","التدفئة","","","dBA","64"]
["Dimensions","Unit","","العرض","mm","600"]
["","","","العمق","mm","1,007"]
["","","","الارتفاع","mm","285"]
["الغلاف","المادة","","","","Galvanised steel"]
["الوزن","الوحدة","","","kg","35"]
["Fan","External static pressure","","عالٍ","باسكال","90"]
["","","","الإسمي","باسكال","77"]
["","","","منخفض","باسكال","64"]
["Power supply","الطور","","","","1~"]
["","Frequency","","","Hz","50"]
["","الاسم","","","","V1"]
["","Voltage","","","V","220-240"]
["Power input","Heating","","Nom.","kW","","0.109"]
["","Cooling","","Nom.","kW","","0.109"]
["مروحة","الضغط الاستاتيكي الخارجي","","عالٍ","باسكال","","70","150","150"]
["","","","منخفض","باسكال","","45","111","92"]
["الغلاف","المادة","","","","","Galvanised steel"]
["الأبعاد","الوحدة","","الارتفاع","mm","","378","378","378"]
["","","","العرض","mm","","541","1300","1500"]
["","","","العمق","mm","","1045","541","541"]
["الوزن","الوحدة","","","kg","","44","50","56"]
["Fan","Air flow rate","Cooling","High","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37","44"]
["","","","Low","m³/min","","18.3","34.8","37.9"]
["","","Heating","High","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37.4","43.9"]
["","","","Low","m³/min","","18.3","34.8","37.9"]
["مروحة","الضغط الاستاتيكي الخارجي","","الإسمي","باسكال","","57","128","122"]
["مستوى طاقة الصوت","التبريد","","","dBA","","60","72","73"]
["","التدفئة","","","dBA","","60","72","73"]
["Sound pressure level","Cooling","","High","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Low","dBA","","36","50","50"]
["","Heating","","High","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Low","dBA","","36","50","50"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","","15.88","15.9","15.9"]
["","التصريف","","","","","19.05"]
["Standard Accessories","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["وحدة التزويد بالطاقة","الطور","","","","","1~"]
["Power supply","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Cooling capacity","Total capacity","","Nom.","kW","","","12.10","13.00"]
["استطاعة التدفئة","الاستطاعة الإجمالية","","الإسمي","kW","","","13.5","15.5"]
["الغلاف","اللون","","","","","","صفائح ستيل مغلفنة / غير مدهونة","صفائح ستيل مغلفنة / غير مدهونة"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","","","37","44"]
["","","تدفئة","متوسط","m³/min","","","37.4","43.9"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","","","52","53"]
["","تدفئة","","متوسط","dBA","","","52","53"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","","","ARCWLA","ARCWLA"]