{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ140DV1","ACQ125DV1"]
["Fan","Air flow rate","Heating","Silent operation","m³/min","15","17.6","22.1","22.1"]
["Power input","Heating","","Nom.","kW","0.067","0.094","0.137","0.137"]
["","Cooling","","Nom.","kW","0.067","0.094","0.137","0.137"]
["Fan","Air flow rate","Cooling","Silent operation","m³/min","15","17.6","22.1","22.1"]
["الغلاف","المادة","","","","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel"]
["الأبعاد","الوحدة","","الارتفاع","mm","265","300","300","300"]
["","","","العرض","mm","820","820","820","820"]
["","","","العمق","mm","820","820","820","820"]
["الوزن","الوحدة","","","kg","31","39","39","39"]
["Fan","Air flow rate","Cooling","High","m³/min","24.4","29.2","34","34"]
["","","","Nom.","m³/min","20.5","24.4","29.2","29.2"]
["","","","Low","m³/min","17.6","21","26.3","26.3"]
["","","Heating","High","m³/min","24.4","29.2","34","34"]
["","","","Nom.","m³/min","20.5","24.4","29.2","29.2"]
["","","","Low","m³/min","17.6","21","26.3","26.3"]
["مستوى طاقة الصوت","التبريد","","","dBA","54","56","60","60"]
["","التدفئة","","","dBA","54","56","60","60"]
["Sound pressure level","Cooling","","High","dBA","41","44","47","47"]
["","","","Nom.","dBA","38","41","44","44"]
["","","","Low","dBA","35","38","43","43"]
["","","","Silent operation","dBA","32","36","41","41"]
["","Heating","","High","dBA","41","44","47","47"]
["","","","Nom.","dBA","38","41","44","44"]
["","","","Low","dBA","35","38","43","43"]
["","","","Silent operation","dBA","32","36","41","41"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.88","15.88","15.88","15.88"]
["","التصريف","","","","19.05","19.05","19.05","19.05"]
["لوحة ديكور","اللون","","","","أبيض","أبيض","أبيض","أبيض"]
["","الأبعاد","","الارتفاع","mm","82","82","82","82"]
["","","","العرض","mm","990","990","990","990"]
["","","","العمق","mm","990","990","990","990"]
["","الوزن","","","kg","4","4","4","4"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","جهاز تحكم عن بُعد سلكي","","","","ARCWB","ARCWB","ARCWB","ARCWB"]
["Standard Accessories","دليل التركيب","","","","دليل التركيب","دليل التركيب","دليل التركيب","دليل التركيب"]
["","جهاز تحكم عن بعد لاسلكي","","","","جهاز تحكم عن بعد لاسلكي","جهاز تحكم عن بعد لاسلكي","جهاز تحكم عن بعد لاسلكي","جهاز تحكم عن بعد لاسلكي"]
["","مشوى بغطاء مع قفل","","","","مشوى بغطاء مع قفل","مشوى بغطاء مع قفل","مشوى بغطاء مع قفل","مشوى بغطاء مع قفل"]
["","بطارية","","","","بطارية","بطارية","بطارية","بطارية"]
["","دليل التشغيل","","","","دليل التشغيل","دليل التشغيل","دليل التشغيل","دليل التشغيل"]
["","مسامير لولبية","","","","مسامير لولبية","مسامير لولبية","مسامير لولبية","مسامير لولبية"]
["","حلقة إحكام الربط","","","","حلقة إحكام الربط","حلقة إحكام الربط","حلقة إحكام الربط","حلقة إحكام الربط"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]