{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C"]
[]
[]
[]
[]
["","","","","","FAQ71CVEB","FAQ100CVEB","FAQ125CVEB"]
["Power input","Heating","","Nom.","kW","0.068","0.061"]
["","Cooling","","Nom.","kW","0.051","0.061"]
["الغلاف","اللون","","","","أبيض صاف","أبيض صاف"]
["","المادة","","","","Resin","Resin"]
["الأبعاد","الوحدة","","الارتفاع","mm","290","340","340"]
["","","","العرض","mm","1050","1200","1200"]
["","","","العمق","mm","238","240","240"]
["الوزن","الوحدة","","","kg","13","17","17"]
["Fan","Air flow rate","Cooling","High","m³/min","18","26"]
["","","","Nom.","m³/min","16","23"]
["","","","Low","m³/min","14","19"]
["","","Heating","High","m³/min","18","26"]
["","","","Nom.","m³/min","16","23"]
["","","","Low","m³/min","14","19"]
["مستوى طاقة الصوت","التبريد","","","dBA","61","65"]
["","التدفئة","","","dBA","61","65"]
["Sound pressure level","Cooling","","High","dBA","45","49"]
["","","","Nom.","dBA","42","45"]
["","","","Low","dBA","40","41"]
["","Heating","","High","dBA","45","49"]
["","","","Nom.","dBA","42","45"]
["","","","Low","dBA","40","41"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9"]
["","التصريف","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","BRC7EB518","BRC7EB518"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Standard Accessories","غطاء البراغي","","","","","غطاء البراغي"]
["","مشابك","","","","مشابك","مشابك"]
["","دليل التركيب والتشغيل","","","","1","1"]
["","لوحة التركيب","","","","لوحة التركيب","لوحة التركيب"]
["","شريط عزل","","","","شريط عزل","شريط عزل"]
["","مسامير لولبية","","","","مسامير لولبية","مسامير لولبية"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220"]