{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-C"]
[]
[]
[]
[]
["","","","","FFQ25C2VEB","FFQ35C2VEB","FFQ50C2VEB","FFQ60C2VEB"]
["Sound pressure level","Heating","High","dBA","31","34","39","43"]
["","","Nom.","dBA","28.5","30.5","34","40"]
["","","Low","dBA","25","25","27","32"]
["","Cooling","Low","dBA","25","25","27","32"]
["","","High","dBA","31","34","39","43"]
["","","Nom.","dBA","28.5","30.5","34","40"]
["Standard Accessories","دليل التشغيل","","","1","1","1","1"]
["","دليل التركيب","","","1","1","1","1"]
["","خرطوم الصرف","","","1","1","1","1"]
["","مشبك معدني لخرطوم الصرف","","","1","1","1","1"]
["","حلقة للدعامة الحاملة","","","8","8","8","8"]
["","مسامير لولبية","","","4","4","4","4"]
["","نموذج ورق للتركيب","","","1","1","1","1"]
["","عازل لأدوات التثبيت","","","2","2","2","2"]
["","لبادة مانعة للتسريب","","","4","4","4","4"]
["","مشابك","","","7","7","7","7"]
["أنظمة التحكم","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية), BRC7EB530 (لوحة قياسية)","BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية), BRC7EB530 (لوحة قياسية)","BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية), BRC7EB530 (لوحة قياسية)","BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية), BRC7EB530 (لوحة قياسية)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.52","9.52","12.7","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","التبريد","","dBA","48","51","56","60"]
["Dimensions","Unit","العرض","mm","575","575","575","575"]
["","","العمق","mm","575","575","575","575"]
["","","الارتفاع","mm","260","260","260","260"]
["الغلاف","المادة","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الوزن","الوحدة","","kg","16","16","17.5","17.5"]
["لوحة ديكور","الوزن","","kg","2.8","2.8","2.8","2.8"]
["","الطراز","","","BYFQ60CW (لوحة بيضاء)","BYFQ60CW (لوحة بيضاء)","BYFQ60CW (لوحة بيضاء)","BYFQ60CW (لوحة بيضاء)"]
["","الأبعاد","الارتفاع","mm","46","46","46","46"]
["","","العمق","mm","620","620","620","620"]
["","","العرض","mm","620","620","620","620"]
["","اللون","","","أبيض (N9.5)","أبيض (N9.5)","أبيض (N9.5)","أبيض (N9.5)"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50"]
["","الاسم","","","VE","VE","VE","VE"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - الأبعاد لا تشمل علبة التحكم","(1) - الأبعاد لا تشمل علبة التحكم","(1) - الأبعاد لا تشمل علبة التحكم","(1) - الأبعاد لا تشمل علبة التحكم"]
["","","","","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]