{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":14,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-B8"]
[]
[]
[]
[]
["","","","","","FHQ35BVV1B","FHQ35BWV1B","FHQ50BWV1B","FHQ50BVV1B","FHQ60BVV1B","FHQ60BWV1B","FHQ71BVV1B","FHQ100BVV1B","FHQ125BVV1B"]
["Power input","Heating","","Nom.","kW","","0.111","0.111","","","0.115"]
["","Cooling","","Nom.","kW","","0.111","0.111","","","0.115"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","195","195","195","195","195","195","195","195","195"]
["","","","العرض","mm","960","960","960","960","1160","1160","1160","1400","1590"]
["","","","العمق","mm","680","680","680","680","680","680","680","680","680"]
["الوزن","الوحدة","","","kg","24","24","25","25","27","27","27","32","35"]
["Fan","Air flow rate","Cooling","High","m³/min","13","13","13","13","17","17","17","24","30"]
["","","","Low","m³/min","10","10","10","10","13","13","14","20","25"]
["","","Heating","High","m³/min","13","13","13","13","16","16","17","24","30"]
["","","","Low","m³/min","10","10","10","10","13","13","14","20","25"]
["مستوى طاقة الصوت","التبريد","","","dBA","53","53","54","54","55","55","55","58","60"]
["","التدفئة","","","dBA","53","53","54","54","55","55","55","58","60"]
["Sound pressure level","Cooling","","High","dBA","37","37","38","38","39","39","39","42","44"]
["","","","Low","dBA","32","32","33","33","33","33","35","37","39"]
["","Heating","","High","dBA","37","37","38","38","39","39","39","42","44"]
["","","","Low","dBA","32","32","33","33","33","33","35","37","39"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35","6.35","6.35","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","9.52","9.5","12.7","12.70","12.70","12.7","15.90","15.90","15.9"]
["","التصريف","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Standard Accessories","حلقة للدعامة الحاملة","","","","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة"]
["","مشبك معدني","","","","مشبك معدني","مشبك معدني","مشبك معدني","مشبك معدني","مشبك معدني","مشبك معدني","مشبك معدني","مشبك معدني","مشبك معدني"]
["","مشابك","","","","مشابك","مشابك","مشابك","مشابك","مشابك","مشابك","مشابك","مشابك","مشابك"]
["","خرطوم الصرف","","","","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف"]
["","دليل التركيب والتشغيل","","","","1","","","1","1","","1","1","1"]
["","عازل لأدوات التثبيت","","","","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت"]
["","نموذج ورق للتركيب","","","","نموذج ورق للتركيب","نموذج ورق للتركيب","نموذج ورق للتركيب","نموذج ورق للتركيب","نموذج ورق للتركيب","نموذج ورق للتركيب","نموذج ورق للتركيب","نموذج ورق للتركيب","نموذج ورق للتركيب"]
["","لبادة مانعة للتسريب","","","","لبادة مانعة للتسريب","","","لبادة مانعة للتسريب","لبادة مانعة للتسريب","","لبادة مانعة للتسريب","لبادة مانعة للتسريب","لبادة مانعة للتسريب"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1","V1","V1","V1","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","دليل التركيب","","","","","دليل التركيب","دليل التركيب","","","دليل التركيب"]
["","دليل التشغيل","","","","","دليل التشغيل","دليل التشغيل","","","دليل التشغيل"]
["","لباد مانع للتسريب","","","","","لباد مانع للتسريب","لباد مانع للتسريب","","","لباد مانع للتسريب"]