{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTN-F"]
[]
[]
[]
[]
["","","","","FTN50FV1B","FTN60FV1B"]
["Sound pressure level","Cooling","Low","dBA","34","36"]
["","","High","dBA","43","45"]
["Standard Accessories","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","2","2"]
["","دليل التشغيل","","","1","1"]
["","دليل التركيب","","","1","1"]
["","البطاريات","","","2","2"]
["","حامل جهاز التحكم عن بعد","","","1"]
["","لوح التثبيت","","","1","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","2","2"]
["","جهاز تحكم عن بعد لاسلكي","","","1","1"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35"]
["","غاز","القطر الخارجي","mm","12.7","12.7"]
["","Drain","","","18","18"]
["Sound power level","التبريد","","dBA","59","61"]
["Dimensions","Unit","العرض","mm","1,050","1,050"]
["","","العمق","mm","238","238"]
["","","الارتفاع","mm","290","290"]
["الغلاف","اللون","","","White","White"]
["الوزن","الوحدة","","kg","12","12"]
["Power supply","الطور","","","1~","1~"]
["","Frequency","","Hz","50","50"]
["","الاسم","","","V1","V1"]
["","Voltage","","V","220-240","220-240"]