{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV / RXL-M"]
[]
[]
[]
[]
["","","","","FTXL25J2V1B / RXL25M2V1B","FTXL35J2V1B / RXL35M2V1B"]
["Cooling capacity","Min.","","kW","1.2","1.3"]
["","Max.","","kW","3.4","3.8"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.5","9.5"]
["","Drain","OD","mm","18","18"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","400.5","570"]
["","نسبة فعالية استهلاك الطاقة","","","3.12","3.07"]
["","عامل الأداء","","","4.43","4.21"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","B","B"]
["","","تدفئة","","A","A"]
["Heating capacity","Min.","","kW","1.1","1.2"]
["","Max.","","kW","5.5","6.0"]
["Notes","","","","(1) - للحصول على الحد الأدنى المقدّر من استطاعة التدفئة يتم ضبط مروحة الوحدة الداخلية إلى العتبة SL","(1) - للحصول على الحد الأدنى المقدّر من استطاعة التدفئة يتم ضبط مروحة الوحدة الداخلية إلى العتبة SL"]
["","","","","(2) - 220 فولت","(2) - 220 فولت"]
["","","","","(3) - 230 فولت","(3) - 230 فولت"]
["","","","","(4) - 240 فولت","(4) - 240 فولت"]
["","","","","(5) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(5) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(6) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(6) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]