{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-B8"]
[]
[]
[]
[]
["","","","","FUQ71BWV1B","FUQ100BWV1B","FUQ125BWV1B"]
["Sound pressure level","Heating","High","dBA","40","43","44"]
["","","Low","dBA","35","38","39"]
["","Cooling","Low","dBA","35","38","39"]
["","","High","dBA","40","43","44"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual"]
["","خرطوم الصرف","","","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف"]
["","مشبك معدني","","","مشبك معدني","مشبك معدني","مشبك معدني"]
["","عازل لأدوات التثبيت","","","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت"]
["","لبادة مانعة للتسريب","","","لبادة مانعة للتسريب","لبادة مانعة للتسريب","لبادة مانعة للتسريب"]
["","مشابك","","","مشابك","مشابك","مشابك"]
["","مسامير لولبية","","","مسامير لولبية","مسامير لولبية","مسامير لولبية"]
["","حلقة إحكام الربط","","","حلقة إحكام الربط","حلقة إحكام الربط","حلقة إحكام الربط"]
["","وصلة","","","وصلة","وصلة","وصلة"]
["","الوح الحامل","","","الوح الحامل","الوح الحامل","الوح الحامل"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.9","15.9","15.9"]
["","Drain","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Power input","Cooling","Nom.","kW","0.180","0.289","0.289"]
["","Heating","Nom.","kW","0.160","0.269","0.269"]
["Sound power level","التبريد","","dBA","56","59","60"]
["","التدفئة","","dBA","56","59","60"]
["Dimensions","Unit","العرض","mm","895","895","895"]
["","","العمق","mm","895","895","895"]
["","","الارتفاع","mm","165","230","230"]
["الغلاف","المادة","","","Resin","Resin","Resin"]
["","اللون","","","White","White","White"]
["الوزن","الوحدة","","kg","25","31","31"]
["Power supply","الطور","","","1~","1~","1~"]
["","Frequency","","Hz","50","50","50"]
["","الاسم","","","V1","V1","V1"]
["","Voltage","","V","220-240","220-240","220-240"]