{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["الغلاف","اللون","","","","أبيض صاف","أبيض صاف","أبيض صاف"]
["","المادة","","","","Resin","Resin","Resin"]
["الأبعاد","الوحدة","","الارتفاع","mm","198","198","198"]
["","","","العرض","mm","950","950","950"]
["","","","العمق","mm","950","950","950"]
["الوزن","الوحدة","","","kg","25","26","26"]
["Fan","Air flow rate","Cooling","High","m³/min","23","31","32.5"]
["","","","Nom.","m³/min","19.5","25.5","26.5"]
["","","","Low","m³/min","16","20","20.5"]
["","","Heating","High","m³/min","23","31","32.5"]
["","","","Nom.","m³/min","19.5","25.5","26.5"]
["","","","Low","m³/min","16","20","20.5"]
["مستوى طاقة الصوت","التبريد","","","dBA","59","64","65"]
["","التدفئة","","","dBA","59","64","65"]
["Sound pressure level","Cooling","","High","dBA","41","46","47"]
["","","","Nom.","dBA","38","42","43"]
["","","","Low","dBA","35","39","40"]
["","Heating","","High","dBA","41","46","47"]
["","","","Nom.","dBA","38","42","43"]
["","","","Low","dBA","35","39","40"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9"]
["","التصريف","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["ارتفاع الصرف","mm","","","","600","600","600"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","BRC7C58","BRC7C58","BRC7C58"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Standard Accessories","دليل التركيب","","","","دليل التركيب","دليل التركيب","دليل التركيب"]
["","حلقة للدعامة الحاملة","","","","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة"]
["","حلقة إحكام الربط","","","","حلقة إحكام الربط","حلقة إحكام الربط","حلقة إحكام الربط"]
["","مادة مانعة","","","","مادة مانعة","مادة مانعة","مادة مانعة"]
["","أنبوب منحني بشكل L","","","","أنبوب منحني بشكل L","أنبوب منحني بشكل L","أنبوب منحني بشكل L"]
["","قماش غير منسوج","","","","قماش غير منسوج","قماش غير منسوج","قماش غير منسوج"]
["","مادة عازلة ومانعة تسريب للوصلات","","","","مادة عازلة ومانعة تسريب للوصلات","مادة عازلة ومانعة تسريب للوصلات","مادة عازلة ومانعة تسريب للوصلات"]
["","دليل التشغيل","","","","دليل التشغيل","دليل التشغيل","دليل التشغيل"]
["","مشبك معدني","","","","مشبك معدني","مشبك معدني","مشبك معدني"]
["","مشابك","","","","مشابك","مشابك","مشابك"]
["","إعلان التوافق","","","","إعلان التوافق","إعلان التوافق","إعلان التوافق"]
["","خرطوم الصرف","","","","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف"]
["","كوع","","","","كوع","كوع","كوع"]
["","نموذج التركيب","","","","نموذج التركيب","نموذج التركيب","نموذج التركيب"]
["","مسامير لولبية","","","","مسامير لولبية","مسامير لولبية","مسامير لولبية"]
["وحدة التزويد بالطاقة","الاسم","","","","VE","VE","VE"]
["","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220"]