{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":9,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Power input","Heating","","Nom.","kW","0.117","0.238","0.238","0.276"]
["","Cooling","","Nom.","kW","0.117","0.238","0.238","0.276"]
["الغلاف","اللون","","","","أبيض صاف","أبيض صاف","أبيض صاف","أبيض صاف"]
["الأبعاد","الوحدة","","الارتفاع","mm","1850","1850","1850","1850"]
["","","","العرض","mm","600","600","600","600"]
["","","","العمق","mm","270","350","350","350"]
["الوزن","الوحدة","","","kg","39","47","47","47"]
["Fan","Air flow rate","Cooling","High","m³/min","18","28","28","30"]
["","","","Nom.","m³/min","16","25","26","28"]
["","","","Low","m³/min","14","22","24","26"]
["","","Heating","High","m³/min","18","28","28","30"]
["","","","Nom.","m³/min","16","25","26","28"]
["","","","Low","m³/min","14","22","24","26"]
["مستوى طاقة الصوت","التبريد","","","dBA","55","62","63","65"]
["","التدفئة","","","dBA","55","62","63","65"]
["Sound pressure level","Cooling","","High","dBA","43","50","51","53"]
["","","","Nom.","dBA","41","47","48","51"]
["","","","Low","dBA","38","44","46","48"]
["","Heating","","High","dBA","43","50","51","53"]
["","","","Nom.","dBA","41","47","48","51"]
["","","","Low","dBA","38","44","46","48"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9","15.9"]
["","التصريف","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Standard Accessories","دليل التركيب","","","","دليل التركيب","دليل التركيب","دليل التركيب","دليل التركيب"]
["","مطاط حماية الفتحات","","","","مطاط حماية الفتحات","مطاط حماية الفتحات","مطاط حماية الفتحات","مطاط حماية الفتحات"]
["","غطاء","","","","غطاء","غطاء","غطاء","غطاء"]
["","مادة حماية من الندى","","","","مادة حماية من الندى","مادة حماية من الندى","مادة حماية من الندى","مادة حماية من الندى"]
["","تمديدات سلكية للتحكم عن بعد","","","","تمديدات سلكية للتحكم عن بعد","تمديدات سلكية للتحكم عن بعد","تمديدات سلكية للتحكم عن بعد","تمديدات سلكية للتحكم عن بعد"]
["","دعامة للتركيب","","","","دعامة للتركيب","دعامة للتركيب","دعامة للتركيب","دعامة للتركيب"]
["","دليل التشغيل","","","","دليل التشغيل","دليل التشغيل","دليل التشغيل","دليل التشغيل"]
["","كم وصل","","","","كم وصل","كم وصل","كم وصل","كم وصل"]
["","مشابك","","","","مشابك","مشابك","مشابك","مشابك"]
["","نموذج التركيب","","","","نموذج التركيب","نموذج التركيب","نموذج التركيب","نموذج التركيب"]
["","عازل لأدوات التثبيت","","","","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت"]
["","مسامير لولبية","","","","مسامير لولبية","مسامير لولبية","مسامير لولبية","مسامير لولبية"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]