{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":10,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / 5MXS-E"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / FTXS20K2V1B / FTXS25K2V1B / FTXS25K2V1B / 5MXS90E3V3B","FTXS20K2V1B / FTXS20K2V1B / FTXS50K2V1B / 5MXS90E3V3B2","FTXS20K2V1B / FTXS35K2V1B / FTXS35K2V1B / 5MXS90E3V3B","FTXS25K2V1B / FTXS25K2V1B / FTXS42K2V1B / 5MXS90E3V3B","FTXS42K2V1B / FTXS50K2V1B / 5MXS90E3V3B","FTXS20K2V1B / FTXS20K2V1B / FTXS50K2V1B / 5MXS90E3V3B"]
["Space cooling","SEER","","","6.43","6.11","6.05","6.11","5.56","6.11"]
["","Annual energy consumption","","kWh/a","424","446","450","450","485","446"]
["","Capacity","Pdesign","kW","7.78","7.77","7.77","7.84","7.70","7.77"]
["","Energy efficiency class","","","A++","A++","A+","A++","A","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.46","5.43","6.35","5.74","4.41","5.43"]
["","SCOP/A","","","4.01","3.89","3.91","3.91","3.84","3.89"]
["","Energy efficiency class","","","A+","A","A","A","A","A"]
["","Annual energy consumption","","kWh/a","2,257","1,953","2,273","2,056","1,607","1,953"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]